LW (from register $t6) = read in a scancode from the keyboard

SW (to register $t7) = send scancode to VGA